**One Point Lesson: Collection of Samples**

1. Remove the current ziplock bag from the sampling port.
2. Sanitize the sampling port with 70% IPA.
3. Place the current ziplock bag in the sampling port.
4. Switch on both the air supply and collect about 1/3 filled with the bag with spray dry powder.
5. Once collected, remove the ziplock bag with 1/3 of the bag filled with spray dry powder and sanitize the sampling port with 70% IPA again and place a new ziplock bag to the sampling port.

Done by: Shahrul Aswad (Intern)